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1、 [bookmark: _Toc7758]System Login
[bookmark: _Toc1706]1.Password Unlock
[image: Screenshot_20260824-092229]

The account is a phone number.
Default Account：18888888888
Default password：123456


2、 [bookmark: _Toc20520]Intelligent Shelving System
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1. [bookmark: _Toc11948]Open-shelf operation
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(1) [bookmark: _Toc23064]Move Left
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[bookmark: _Toc1456][image: mipmap-mdpi_首页]
2. [bookmark: _Toc5837]Close-shelf operation
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1. [bookmark: _Toc18765]Area Col Set
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[bookmark: _Toc29930](1)Position Parameters
1)Columns in Zone
2)Group Per Columns
3)Layers Per Group
4)Boxes Per Layer
5)Arrangement Order
You can set three sorting modes: left‑to‑right, middle‑fixed, and right‑to‑left.
6)Fixed Column No
7)Fixed Column Position
Fixed column positioning can be configured in three ways: left fixed, center fixed, or right fixed.
[bookmark: _Toc9478](2)Running Parameters
1)Running Speed
Set operating speed: High, Medium, Low
2)Running Time
Set a maximum operation time; if the scaffold is not in place beyond this time limit, a timeout alarm will be triggered, and the scaffold will stop.
3)Aisle Width
The maximum travel distance setting prevents derailment; if the scaffold exceeds this maximum distance, an over-distance alarm will be triggered, and the scaffold will stop.

2. [bookmark: _Toc18757]Advanced
[image: Screenshot_20260824-092303]
[bookmark: _Toc5762](1)Timing Settings
Enable automatic sleep mode; set the duration before automatic sleep upon idle period; set the duration before automatic logout upon idle period; enable automatic reboot at midnight.
[bookmark: _Toc14799](2)Information Settings
Whether the welcome message on the login page is enabled and the content of the welcome message; settings for the company name on the homepage, the system name, and the logo.
[bookmark: _Toc17422](3)Other Settings
Serial port baud rate configuration and whether the system log is enabled.
3. [bookmark: _Toc18768]User Mgmt
[image: Screenshot_20260824-092307]
The administrator account can modify, disable, or delete users.
[bookmark: _Toc3130](1)Add User
[image: Screenshot_20260824-092855]
Add a new user: set a username, account (an 11-digit phone number), and password.




4. [bookmark: _Toc20315]Support
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[bookmark: _Toc5769](1)Hardware Config
[bookmark: _Toc12985](2)Software Version
[bookmark: _Toc24236](3)Hardware Version
[bookmark: _Toc6202][bookmark: _GoBack](4)Tel
[bookmark: _Toc13964](5)E-mail
[bookmark: _Toc12564](6)Web
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